===============================================================================
License Agreement
===============================================================================

The license agreement for this software (hereinafter referred to as the
SOFTWARE) is described as follows.

1. Intellectual property rights in the SOFTWARE shall remain in Fuji Xerox Co.,
   Ltd. (hereinafter referred to as Fuji Xerox) as well as the original
   copyright holders.

2. The SOFTWARE can only be used with compatible Fuji Xerox products
   (hereinafter referred to as the COMPATIBLE PRODUCTS) within the country of
   purchase of the COMPATIBLE PRODUCTS.

3. You are required to abide by the notes and restrictions (hereinafter referred
   to as the NOTES AND RESTRICTIONS) declared by Fuji Xerox while using the
   SOFTWARE.

4. You are not permitted to alter, modify, reverse engineer, decompile or
   disassemble the whole or any part of the SOFTWARE for the purpose of
   analyzing the SOFTWARE.

5. You are not permitted to distribute the SOFTWARE on a communication network,
   or transfer, sell, rent or license the SOFTWARE to any third party by
   duplicating the SOFTWARE on any media such as floppy disk or magnetic tape.

6. Fuji Xerox, Fuji Xerox Channel Partners, Authorized Dealers and the original
   copyright holders of the SOFTWARE shall not be liable for any loss or damage
   arising from matching of hardware or program that are not specified in the
   NOTES AND RESTRICTIONS of the SOFTWARE, or any modification to the SOFTWARE.

7. Fuji Xerox, Fuji Xerox Channel Partners, Authorized Dealers and the original
   copyright holders of the SOFTWARE shall not be responsible for any warranty
   or liability with respect to the SOFTWARE.

===============================================================================
Multi-model Print Driver 2 Ver.2.7.18 Additional Information
===============================================================================

This document provides information about the driver on the
following items:

1. Requirements
2. Installation
3. Version Improvements
4. General Comments
5. Limitations
6. Software Update

---------------------------------------------------
1. Requirements
---------------------------------------------------
1.Please note that this driver operates on a computer running on the following
  operating system.

  Microsoft(R) Windows Vista(R) x64 Editions
  Microsoft(R) Windows Server(R) 2008 x64 Editions
  Microsoft(R) Windows(R) 7 x64 Editions
  Microsoft(R) Windows Server(R) 2008 R2
  Microsoft(R) Windows(R) 8 x64 Editions
  Microsoft(R) Windows Server(R) 2012
  Microsoft(R) Windows(R) 8.1 x64 Editions
  Microsoft(R) Windows Server(R) 2012 R2
  Microsoft(R) Windows(R) 10 x64 Editions
  Microsoft(R) Windows Server(R) 2016

  Also, to check the models corresponding to this driver, refer to the
  following URL.

  For customers in the Asia Pacific region excluding Japan:

      https://www.fujixerox.com/

  For customers in Japan:

      https://www.fujixerox.co.jp/

  Please visit our web site to check the latest software and supported
  operating systems.

2.Some softwares related to the driver installation are attached to the
  driver package. Please refer to EzInst\Readme.htm about them.

---------------------------------------------------
2. Installation
---------------------------------------------------
Follow the instructions below to install Multi-model Print Driver 2.

Notice:
  * Close all the running applications before installing the print driver.
  * Always reboot the computer after installing an upgraded version of the
    print driver.
  * If you have deleted an older version of the print driver, always reboot
    the computer before installing the new version.
  * For Plug and Play driver installation on Windows 7, Windows Server 2008 R2,
    Windows 8, Windows Server 2012, Windows 8.1, Windows Server 2012 R2 or
    Windows 10.
    Please refer to the following chapter.
    "About driver installation method using plug-and-play
    (When using Windows 7, Windows Server 2008 R2, Windows 8,
    Windows Server 2012, Windows 8.1, Windows Server 2012 R2 or Windows 10)"

2.1 Installation on Windows Vista x64 Edition, Windows Server 2008 x64 Edition,
    Windows 7 x64 Edition, Windows Server 2008 R2 
===============================================================================

(1) 1a) For Windows Vista, windows Server 2008, follow steps below
        Start > Control Panel > Select [Printer] in Hardware Wizard.

    1b) For Windows 7 or Windows Server 2008 R2, follows steps below
        Start > Device and Printer > Select [Add a Printer] in Device and
        Printer

(2) Select [Add a printer] from the menu bar.
    (Windows Server 2008:[Run as Administrator] > [Add Printer])

(3) Click [Next>].
    If the printer is directly attached to your computer or is connected to the
    Network using the LPR protocol, choose [Add a local printer], then click
    [Next>] and follow the instructions from (5).
    Otherwise, choose [Add a network, wireless or Bluetooth printer].

(4) Select [The printer that I want isn't listed].
    Connect to the desired printer by one of the method:
    * Select [Browse for a printer] button, and then click [Next>] to locate
      the printer on the network.
    * [Select a shared printer by name] button to type the name using
      the following format.

      \\printserver_name\share_name

    Then follow the instructions from (11).
    If you are not familiar with the network, please consult the network
    administrator.

(5) Select the printer port where the printer device is connected directly,
    click [Next>], and go to step (7).
    If the printer is connected to the Network using the LPR protocol,
    select [Standard TCP/IP Port] of the [Create a new port:] section,
    and then click [Standard TCP/IP port].

(6) Enter the Hostname or IP address in the [Hostname or IP Address] edit box.
    If you do not know the Hostname or IP address, please consult the network
    administrator.

(7) Click [Have Disk....] in the [Add Printer Wizard] and specify a folder in
    which the driver files are. Then select the INF file in the folder and then
    click [OK].

(8) [Multi-model Print Driver 2] appears in the dialog box. Select the printer
    and click [Next].
    If the selected printer is already installed, a message asking whether to
    replace the existing driver is displayed.
    When installing a new version of the print driver, select [Replace the
    current driver]. The older version of the driver cannot be deleted if it is
    used in an application.
    In this case, close the application.

(9) A dialog box for specifying the printer name is displayed.
    To change the printer name, enter any name in the [Printer name] box.
    If other printers are installed, a message asking whether to make this the
    default printer is shown.
    Confirm that [Set as the default printer] is selected.

(10) [User Account Control] dialog will be displayed and ask if you continue
     [Change Printing Settings]. Click [Continue].
     When executing installation as a user other than Administrator,
     password for Administrator is required.

(11) Installation starts. A message saying that Windows can't verify
     the publisher of this driver software will be displayed but this does not
     cause functional problem. Click [Install this driver software anyway] to
     continue the installation.

(12) A dialog box specifying whether to print the test page after installation
     is shown. Click [Print a test page] button to print the test page.
     Otherwise, click [Finish] if you do not wish to print the test page.

2.2 Installation on Windows 8 x64 Edition, Windows Server 2012,
    Windows 8.1 x64 Edition, Windows Server 2012 R2, Windows 10 x64 Edition
===========================================================================

(1) Go to Control Panel > [Hardware and Sound] > [Devices and Printers].

(2) Select [Add a printer] from the menu bar.

(3) Specify the printer connection.
    * For a local printer:
      Specify the local printer going through the menu displayed on Windows.
      Proceed to Step (4)
    * For a network printer:
      Specify the desired printer from the network going through the menu
      displayed on Windows.
      Contact the network administrator if you have any queries.
      If other printers are installed, a message asking whether to set this as
      the default printer is shown. Click [Yes] if you want to set it as a
      default printer.
      Proceed to step (8).

(4) Specify the printer port. Create a port if there is no output port.
    Please refer to the [Frequently Asked Questions] from our driver download
    page for the port creation method.

(5) Specify the printer model. Click [Have Disk...] to display the [Install
    From Disk] dialog box.
    Select a folder in which the driver files are. Then select the INF file in
    the folder and then click [OK].

(6) [Multi-model Print Driver 2] appears in the dialog box. Select the printer
    and click [Next].
    If the selected printer is already installed, a message asking whether to
    replace the existing driver is displayed.
    When installing a new version of the print driver, select [Replace the
    current driver]. The older version of the driver cannot be deleted if it is
    used in an application.
    In this case, close the application.

(7) A dialog box for specifying the printer name is displayed.
    To change the printer name, enter any name in the [Printer name] box.

(8) Installation starts.
    * [User Account Control] dialog will be displayed and ask if you continue
      [Change Printing Settings]. Click [Continue].
      When executing installation as a user other than Administrator,
      password for Administrator is required.
    * The installation confirmation screen published by Fuji Xerox Co., Ltd.
      may be displayed, but it is not a functional problem.
      Click [Install].

(9) A dialog box specifying whether to print the test page after installation
    is shown. Click [Print a test page] button to print the test page.
    Otherwise, click [Finish] if you do not wish to print the test page.

2.3 Uninstallation on Windows Vista x64 Edition,
    Windows Server 2008 x64 Edition, Windows 7 x64 Edition,
    Windows Server 2008 R2, Windows 8 x64 Edition, Windows Server 2012,
    Windows 8.1 x64 Edition, Windows Server 2012 R2, Windows 10 x64 Edition
===========================================================================

For Windows Vista, Windows Server 2008.
  * Click [Start] button, open [Control Panel], then select [Printer] in
    [Hardware and Sound].
  * Delete the printer icon in the [Printer] folder.
  * Right-click on the [Printer] folder, go to [Run as administrator] ->
    [Server Properties] and display [Print Server Properties].
  * Select the driver to be deleted on the [Driver] tab and click the
    [Remove] button.
  * Select [Remove driver and driver packages] and click [OK].
  * Reboot the computer.

For Windows 7, Windows Server 2008 R2.
  * Click [Start] button, then select [Device and Printer].
  * Delete the printer icon in the [Device and Printer] folder.
  * Select any icon displayed in the [Printer and Fax] from inside of
    [Device and Printer] folder, then select [Printer Server Properties].
  * Click the button [Change Driver Settings].
  * Select the driver to be deleted on the [Driver] tab and click the
    [Remove] button.
  * Select [Remove driver and driver packages] and click [OK].
  * Driver packages may not be removed while driver is being used, retry
    after reboot the computer.
  * Reboot the computer.

For Windows 8, Windows Server 2012, Windows 8.1, Windows Server 2012, Windows 10.
  * Go to [Control Panel] > [Hardware and Sound] > [Devices and Printers].
  * Delete the printer icon in the [Device and Printer] folder.
  * Select any icon displayed in the [Printer] from inside of 
    [Device and Printer] folder, then select [Printer Server Properties].
  * Click the button [Change Driver Settings].
  * Select the driver to be deleted on the [Driver] tab and click the
    [Remove] button.
  * Select [Remove driver and driver packages] and click [OK].
  * Driver packages may not be removed while driver is being used, retry
    after reboot the computer.
  * Reboot the computer.

About driver installation method using plug-and-play
(When using Windows 7, Windows Server 2008 R2, Windows 8, Windows Server 2012,
Windows 8.1, Windows Server 2012 R2 or Windows 10)
-----------------------------------------------------
When a driver is installed using plug-and-play, it may not
be installed properly. In such case, follow the steps below to reinstall
the driver.
  * Select [Device and Printer].
  * Right click on the printer icon in the [Device and Printer] folder,
    them, select [Properties].
    Reboot the computer in case of the icon is dimmed out.
  * Select the printer icon in the [Device Function] in [Hardware] tab,
    then, open properties dialog by clicking [Properties] button.
  * A new [Properties] dialog is opened by click [Change Settings] button.
  * Open [Driver] tab from the new [Properties] dialog box, click
    [Update Driver], [Update Driver Software] dialog will be opened.
  * Select [Browse my computer for driver software], [Serch for driver
    software in this location] specific driver files location you want to
    install then, click [Next].
  * Click [Close] button when driver has been updated message displayed, to
    complete reinstallation.

2.4 How to Update
==============================================================================

The procedure below describes how to update Multi-Print Driver 2 under
the environment where it is already installed.

For Windows Vista and Windows Server 2008
  * Go to [Start] > [Control Panel] and select [Printers] in [Hardware and
    Sound].
  * In [Printers], right-click to select [Run as administrator] >
    [Server Properties] > [Print server properties]. 
  * At [Drivers] tab, click [Add].
  * [Add Printer Driver Wizard] automatically appears. Then, click [Next].
  * Make sure that the checkbox for [x64] is selected and then click [Next].
  * Click [Have Disk...] and specify the folder in which the driver file is
    stored.
    In the folder, select INF file and then click [OK].
  * Choose the driver that you want to install and then click [Next].
  * Click [Finish] in [Add Printer Driver Wizard]. 
  * On [Print server properties] screen, click [OK].
  * Restart your PC.

For Windows 7 and Windows Server 2008 R2
  * Select [Start] > [Devices and Printers].
  * Click any object shown under [Printers and Faxes] in [Devices and Printers].
    With the object put in selected state, select [Print server properties].
  * [Print server properties] screen opens. On this screen, click [Change Form
    Settings].
  * At [Drivers] tab, click [Add].
  * [Add Printer Driver Wizard] appears. Then, click [Next].
  * Make sure that the checkbox for [x64] is selected and then click [Next].
  * Click [Have Disk...] and specify the folder in which the driver file is
    stored.
    In the folder, select INF file and click [OK].
  * Choose the driver that you want to install and then click [Next].
  * Click [Finish] in [Add Printer Driver Wizard]. 
  * On [Print server properties] screen, click [OK].
  * Restart your PC.

For Windows 8, Windows Server 2012, Windows 8.1, Windows Server 2012 R2,
and Windows 10
  * Select [Control Panel] > [Hardware and Sound] > [Devices and Printers].
  * Click any object shown under [Printers] in [Devices and Printers].
    With the object put in selected state, select [Print server properties].
  * [Print server properties] screen opens. On this screen, click [Change Form
    Settings].
  * At [Drivers] tab, click [Add].
  * [Add Printer Driver Wizard] appears. Then, click [Next].
  * Make sure that the checkbox for [x64] is selected and then click [Next].
  * Click [Have Disk...] and specify the folder in which the driver file is
    stored.
    In the folder, select INF file and then click [OK] .
  * Choose the driver that you want to install and click [Next].
  * Click [Finish] in [Add Printer Driver Wizard].
  * On [Print server properties] screen, click [OK].
  * Restart your PC.

---------------------------------------------------
3. Version Improvements
---------------------------------------------------
[Improvements from Ver 2.7.14]
* Indonesian are supported.
* Streamlined the file access processing.
* Improved the phenomenon that printing may fail with EMF Spooling specified in
  a certain environment.

[Improvements from Ver 2.7.13]
* Extended the range of paper size allowed to be specified as custom paper size.

[Improvements from Ver 2.7.12]
* Fixed the problems below, which might occur at printing pages including
  image data in the environment where Security Update Program published by 
  Microsoft on August 9, 2017 (Security Update Program of August 2017) is
  applied.
    - Page is output as a blank page.
    - Output image is partly missing.
    - Unable to output because the size of spool data becomes too large.
* Fixed the problem that characters rotated by +90 degrees/-90 degrees 
  with respect to a document direction may not be printed normally.

[Improvements from Ver 2.7.10]
* Allowed use of combination of "EMF spooling" and the features below on the
  64-bit machine.
    Accounting
    Secure Print, Sample Print, Delayed Print
    Notify Job Completion by E-mail
    Separators

[Improvements from Ver 2.7.8]
* Fixed the problem that when a paper size is changed from an application, 
  the size may not be reflected properly.
* Import of Saved Settings file created using version 2.7.7 or earlier 
  is now supported.
* Fixed the problem that when a document titled in a language other than 
  local OS language is printed, the file name on the job confirmation screen 
  of printer may be garbled.
* Fixed the problem that an error may occur when printer is shared.
* Modified to support Package-Aware.  In the shared printer environment,
  Administrator rights necessary for printer driver installation may not be
  required.

[Improvements from Ver 2.7.7]
* An environment where the languages of OS are different between Server and
  Client is supported.
* Thai and Vietnamese are supported.
* The feature of replacing TrueType font with the printer font or other
  TrueType fonts to output is supported.

[Improvements from Ver 2.7.6]
* UTF-8 is supported.  (See the page of target models for information about
  the UTF-8 support models.)
* Combined use of "Multiple-Up" and "Booklet Creation" features is supported.
* Specifying "Output Method" is supported.

[Improvements from Ver 2.7.4]
* Supported Windows(R) 8.

[Improvements from Ver 2.7.1]
* "Adjust Clip Coordinate" feature is supported.
* Fixed the problem that an error would occur when printing started from a
  certain multithread application

[Improvements from Ver 2.7.0]
* Supported Windows(R) 7.

---------------------------------------------------
4. General Comments
---------------------------------------------------
* Close all the running applications before installing the print driver.

* Always reboot the computer after installing an upgraded version of the print
  driver.

* If you have deleted an older version of the print driver, always reboot the
  computer before installing the new version.

* Some applications provide printing options pertaining to the number of copies
  and collated copies. Always select the printing options in the application
  unless the instructions specify otherwise. Use the print driver dialogs to
  select advanced options such as 2 Sided Print, Sample Set or options that
  are not available in the application.

* Always close the print driver dialogs and/or the application Print dialog box
  before you make any changes to the default settings of the print driver via
  the Control Panel.

* If your Job Offset output does not work well with the collated copies, you
  may try to deselect the [Collate] option in the application and check the
  [Collate] check box in the print driver.

* For the installation through the networks, if you right-click
  on [Printer] folder, go to [Run as administrator] from the menu and select
  [Add printer...], printer icon may not be generated.

* Rename a Printer Icon should comply OS file naming convention. Use Symbols or
  special characters may incur renaming error or unexpected print driver
  behavior.

* Before installing a print driver in the Windows cluster environment, you need
  to install it on each node in the cluster.

---------------------------------------------------
5. Limitations
---------------------------------------------------
* Modified to support Package-Aware.  In the shared printer environment,
  Administrator rights necessary for printer driver installation may not be
  required.

* Support of Package-Aware with Microsoft WHQL Certified Driver
  In the Server-Client environment, if the driver is not Microsoft WHQL
  Certified Driver, when the printer driver is added or upgraded on the Server
  side, a dialog prompting user to install the printer driver or the User
  Account Control dialog may be displayed on the Client side.

* When a printed pattern, diagram, color density or lines are different from
  what you see on the screen, changing the following settings may alleviate the
  problem.

  - Change the [Image Quality] setting on the [Image Options] tab.
  - Set [High Speed Image Processing] on the [Advanced Settings] tab to [Off].
  - Set [Draw the pattern with fine lines as per the resolution] on the
    [Advanced Settings] tab to [On].
  - Change the [Resolution] setting on the [Advanced Settings] tab.
  - Change the [Halftone Print] setting on the [Advanced Settings] tab.

* Blank Separators
  If you set [EMF Spooling] to [Enabled] and perform [2-Sided Print] with documents
  of odd number of pages, a blank page may be inserted on the last page depending
  on application or OS.

* Depending on the application, if the [Image Quality] is [High Resolution] or
  [High Quality] or the resolution of the driver is [600dpi] or [Print Page
  Mode] is [On], the size of the print data may become huge and printing cannot
  be done properly. When this happens, specify the following settings:

  - Specify the [Image Quality] to [Standard] in the [Image Options] tab or
    [Resolution] in the [Other Settings (Graphics Settings)] in the [Advanced
    Settings] tab to [300dpi] or [200dpi].

* When printing from the application of Microsoft Visio 2003, if the [Image
  Quality] setting is changed from [Standard] to [High Resolution] before
  printing, data may be scaled down and printed in the upper left corner.
  This issue can be avoided by setting [Image Quality] to [High Resolution] in
  the [Image Options] tab of the print driver before starting the application.

* When doing a print job by specifying Paper Source as Auto, be sure to set
  Paper Size in the application to the Paper Size that the driver supports to
  enable the automatic paper feed feature.

* The print result may overlap if Multiple Up and Print Area [Normal] are
  selected when printing a document that has exceeded the print area of the
  print driver. When this happens, select the [Print to Edge] in the [Print
  Area] dialog box in the [Image Shift/Print Position] in the [Layout] tab.

* Depending on the application used by the customer, blank pages for page
  adjustment will be inserted automatically according to the conditions like
  the number of copies specified when outputting 2-sided prints.
  In this case, the blank inserts will be included by the application.
  The performance may be improved by changing the setting below.
  - Check [Skip Blank Pages] on [Advanced Settings] tab.
  But the print layout may be changed.

* Even with [Skip Blank Pages] selected, blank pages may still be printed in
  the following situations.
  - The page contains only line feeds.
  - The page contains only spaces.
  - The page contains only line feeds and spaces.
  - A white background drawing instruction is sent from the application.

* With Microsoft Word, even if [Skip Blank Pages] is specified, when a blank
  page is included in documents, it may be output.

* For customers using Microsoft Windows Server 2008 and
  Microsoft Windows Server 2008 R2 Cluster Environment

  <1> To specify custom paper size in a cluster environment, specify a common
      setting for all physical nodes in the cluster environment.

  <2> When [Search Printer] dialog box appears at the press of the [Get
      Information from Printer] button, enter the printer network address.

  <3> Deleting driver in cluster environment
      After the driver on the virtual server is deleted, delete the drivers on
      all standby nodes.

      * Deleting driver from the standby node
        (1) Change the standby node to active node.
        (2) Install printer on virtual server.
        (3) Delete driver from virtual server.

  <4> Deleting driver
      After the printer icon is deleted, delete the driver from [Server
      Properties]. Then, restart the computer.

* [Cancel] button on [Enter User Details] Dialog
  For some applications, if [Enter User Details] dialog is cancelled when
  printing with the settings of [Prompt User for Entry when Submitting Job] on
  [User Details Setup] dialog, a warning dialog may be displayed.
  This warning dialog may indicate a printer error, however, the printer
  actually has no problem.
  In that case, ignore the warning and continue.

* Functional Limitations of EMF Spooling
  When [EMF Spooling] of [Advanced Settings] tab is set to [Enabled],
  the following features may not function normally.
  To use these features, set [EMF Spooling] to [Disabled].
  - [Secure Print][Sample Set][Delayed Print]
  - [Enable Account Setup][User Details Setup]
  - [Notify Job Completion by E-mail]
  - [Annotation]
  - [Insert Separators] of [Covers / Separators]
  - [Use Extended Features From Application]
  - [Enable User Defined Margins]

  When [EMF Spooling] of [Advanced Settings] tab is set to [Disabled],
  some documents with complex structure may have troubles such as distorted
  output image and failure of the output.

* To change the settings of Custom Paper Size, you need the Administrator's
  access rights.

  On Windows Vista or Windows Server 2008, select printer from the printer
  folder, right-click to go [Run as administrator] and select [Properties].
  After clicking [Continue] in [User Account Control], you can change the
  settings from Property.

  On Windows 7 or later versions, select a printer from the [Devices and
  Printers] folder. Select Property of the printer and click the [Change
  Sharing Options] button on the [Sharing] tab.
  Then, specify Custom Paper Size.

* With the default settings of Firewall, data in cross-subnet broadcast cannot
  be retrieved.
  For cross-subnet data retrieval, please do not use broadcast and specify
  address directly.

* Features of printing with Annotation and Watermark
  On Windows 8 or later versions, Annotation and Watermark may not be printed
  even if [Annotation] and [Watermarks] are specified.
  To make them function, set [EMF Spooling] to [Enabled] on the [Advanced
  Settings] tab.

* Annotation features
  In Windows Vista and Windows Server 2008 environments, when [EMF Spooling] of
  [Advanced Settings] tab is set to [Disabled], [Annotation] is not available
  for use by 32bit application software.
  To use this feature, set [EMF Spooling] to [Enabled].

* An installation by specifying the installation file belonging a shared print
  driver, the installation may not be normally completed.
  It is recommended that you perform the installation on local machine after
  copying the install file.

* At [Get Information from Printer] in the [Configuration] tab, the printer
  configuration for some models may not be updated correctly. In this case,
  configure the settings manually.

* The default [Halftone Print] of this driver is set to ON. However, other
  model dedicated drivers may have default [Halftone Print] as OFF.
  Therefore, when the [Output Color] of this driver is set to [Black & White],
  the shading of gray may be printed differently, if comparing the output to the
  one by a model dedicated driver, of which [Halftone Print] is set to OFF by
  default.

* Some characters, line thickness or density of patterns may be printed
  differently from the one by a model dedicated driver.

* Output may be printed differently from the one by a model dedicated driver,
  due to a difference of their image processing methods.
  Such differences include color changes, extra lines, or misalignment.
  To avoid any problems caused by the differences, use a model dedicated driver.

* With the following models, the output is always equivalent to [Print Page Mode]
  regardless of the settings of Image Quality.
  Therefore, some applications or files may take a longer time to output a print
  job depending on the printer.

  DocuCentre-II C5400/C6500/C7500
  ApeosPort-II C5400/C6500/C7500
  DocuCentre-II C2200/C3300/C4300
  ApeosPort-II C2200/C3300/C4300
  DocuCentre-III C2201/C2200/C3300
  ApeosPort-III C2201/C2200/C3300
  DocuCentre-III C4400
  ApeosPort-III C4400
  DocuCentre-III C3100/C4100
  DocuCentre-II 6000/7000
  ApeosPort-II 6000/7000
  DocuCentre-II 4000/5010
  ApeosPort-II 3000/4000/5010
  DocuCentre-II 2005/2055/3005
  DocuCentre-III 2007/3007
  DocuPrint C4350
  DocuPrint C2255

  Note that the above models in Japan are not supported by
  Multi-model Print Driver 2.

* You cannot change the font setting because it is internally set to [Always Use
  True Type Fonts] as a fixed processing in this driver.
  Therefore, some characters may have their thickness and shape printed
  differently when comparing the output to the one with [Substitute True Type
  Fonts with Printer Fonts] setting by a model dedicate driver.
  To avoid any problems caused by the differences, use a model dedicated driver.

* For some models, the following are some restrictions for User ID and Job Name
  that are used in Secure Print, Sample Print, Delayed Print, Charge Print,
  Private Charge Print. You cannot use Japanese kanji or hiragana. The maximum
  number of characters, and the character type  that can be used vary according
  to the models. Please check the maximum number of characters, and the
  character type that can be used in the user guide for your printer.

* Some features, which are available with a model dedicated driver are not
 provided by this driver.

* The following paper sizes are available with this driver.
  - Standard:
    A3(297x420mm), A4(210x297mm), A5(148x210mm), B4(257x364mm),
    B5(182x257mm), Letter(8.5x11"), Legal(8.5x14"), Tabloid(11x17"),
    Postcard(100x148mm)
    
  - Nonstandard:
    Short edge(89~297mm) x Long edge(98~432mm)

* The following paper types are available with this driver.
  Paper Tray: Plain
  Bypass Tray: Plain, Heavyweight, HW Reload, Extra HW, X-HW Reload, Custom

* If the [Secure Print], [Sample Set] or [Delayed Print] job is sent to a
  printer that does not have a Hard Disk option, the print job may be cancelled
  by the printer.

* If the driver specifies 2 Sided Print setting, but the print job is sent to a
  printer, which is not equipped with a Duplex Module, the 2 Sided Print setting
  will be ignored.

* If the driver specifies a paper tray for printing, but the print job is sent
  to a printer, which is not equipped with the specified paper tray, the job
  will be cancelled by the printer.

* A black and white model always outputs a job in black and white, regardless
  of the Output Color settings.

* Except for some models, installation by Plug & Play is not supported.

* Installing network printer in Microsoft Windows Vista and
  Microsoft Windows Server 2008
  When installing network printer by [Run as Administrator], the printer may be
  added under the administrator account used for installation and not under the
  current user.

* Number of Copies
  This driver allows you to print from 1 to 999 copies.
  Only one copy may be printed if the number of copies specified exceeds this
  range.

* Black/Color Auto Recognition
  When [Color (Auto)] is specified at [Output Color], though the output may
  appear to be in black, it has been processed in color. If you are sure that
  you want to print in black, specify [Black] at [Output Color].
  Documents will be printed in color in the following situations.
  - When black and white objects are overlapping the color objects
  - When there are color objects outside the print area
  - When the application uses the system's ICM function to perform color change
  - When the application has its own color change function

* Favorites
  When only a margin setting is changed, [Change] is not displayed in the
  [Favorites] combo box.

* In some applications, when the line width is set to thin lines, the selected
  dotted lines may be printed as solid lines instead.
  If this happens, select another line width.

* Corel DESIGNER
  Objects that are drawn in solid lines may be printed in dotted lines.
  The print output may not look good, for example, lines and gaps may be seen
  in circle gradations.
  The print output may be improved by converting the gradations to images.

* JUSTSYSTEM Ichitaro
  Sometimes the partial printing may not be performed properly.
  Such cases can be avoided by the following method.
  - Before starting the application, open the default setting of the
    document from the Printer Folder and click [OK].

* Microsoft Excel
  When printing a book or multiple sheets in Excel, the second and subsequent
  sheets may not be printed as specified in the dialog settings.
  When you specify to print an entire book with mixed double-sided and
  single-sided sheets, each sheet is printed according to its individual print
  information. Batch printing is not performed.
  You can avoid this problem by doing the following:

  1. Select another printer on the print dialog or page setup dialog of any
     sheet and close the document temporarily to activate the change.
  2. Change the default value of the driver to the desired setting.
     (E.g. 2 Sided Print, 2 Up, etc.)
  3. Open the document and select this driver on the print dialog before
     printing.

  The print layout may be changed when you change the [Resolution] of this
  driver.

  You may not be able to print if you change the port after installing this
  driver. In this case, delete the driver.
  Specify the desired port and install again.

* Microsoft Word
  Even if [Skip Blank Pages] is specified, when a blank page is included in
  documents, it may be output.

  When [Poster] is selected to print two or more copies of a single-page
  document, the copies will not be collated.

  You may not be able to print if you change the port after installing this
  driver. In this case, delete the driver.
  Specify the desired port and install again.

* Color Mode Settings from Application
  To print in color from Application of Windows Store, open [Devices and Printers]
  from Windows Desktop, right-click on your printer to select [Print Settings]
  and then confirm that [Output Color] on the [Paper/Output] tab of the
  [Default Setting] dialog is set to [Color].
  If the setting of [Output Color] on the [Paper/Output] tab of the [Print Settings]
  dialog remains [Black & White], the output will be in black and white even
  if you specify [Color Mode] to [Color] on the printing setting screen shown
  after you select printer from the device charm.

* For models that do not support paper color, the Paper Color settings will be
  ignored even if it is specified.

* For models that do not support Delayed Print or Charge Print related features,
  these features will not be available. Please check the support status in the
  user guide for your printer.

* If printing with [Collated] and multiple [Quantity] settings, there must be
  internal hard disk and RAM disk feature in the multifunction device/printer
  to use the spool feature in the device. If these settings are not available,
  the quantity setting will be ignored.

* For models that feed paper from the front, the paper feed orientation
  specified for Bypass Tray (Portrait/Landscape) is the reverse of the actual
  paper feed orientation.

---------------------------------------------------
6. Software Update
---------------------------------------------------
  The latest software is available on our web site.

  For customers in the Asia Pacific region excluding Japan, the latest
  software is available on our web site.

      https://www.fujixerox.com/

  For customers in Japan:

      https://www.fujixerox.co.jp/

  Communication charges will be borne by the customer.

-------------------------------------------------------------------------------
Microsoft, Windows, Windows Server, Windows Vista, Word, Excel, PowerPoint,
Internet Explorer and Visio are either registered trademarks or trademarks
of Microsoft Corporation in the United States and/or other countries.

Adobe, Acrobat and Reader are either registered trademarks or trademarks of
Adobe Systems Incorporated in the United States and/or other countries.

CentreWare is a registered trademark of Xerox Corporation.

Other company names and product names are trademarks or registered
trademarks of the respective companies.

libjpeg 6b
----------
This software is based in part on the work of the Independent JPEG Group.

(C) Fuji Xerox Co., Ltd. 2009-2019
